COURSE NEEDS AND SUPPORT INFORMATION

Instructional Materials

The following documents can be downloaded from the BLM National Fire Training and Workforce Development website (<https://www.nifc.gov/about-us/our-partners/blm/training/fire-vehicle>)**.**

* 1 per each instructor and course coordinator – *ENOP Facilitator Guide*
* 1 per each instructor and student – *ENOP Student Workbook*
* 1 per each instructor and student – *ENOP Vehicle Inspection Job Aid*

Classroom Audiovisual Equipment

* 1 each – computer
* 1 each – multi-media projector and associated cables
* 1 each – screen

Classroom Supplies

* Name tags and name tents
* Dry erase board (if available)
* Dry erase markers (if dry erase board is available)
* Flipcharts with stands and pads
* Office supplies (as needed)

Extension cords (as necessary for classroom and breakout room)

Outside Exercises Supplies

The fire apparatuses used for the walk through inspections will be gathered from what the students brought to the class. Additional items can be acquired through local unit and local fire cache.

* 1 each – Type 4 engine
* 1 each – Type 6 engine
* 1 each – Type 3 engine (optional)
* 1 gallon – environmentally-safe antifreeze
* Parking lot or field near classroom to park engines for inspections
* Air compressor or air hose off engine air tank (winterization station)
* Parking lot or field near classroom and large enough to set up cone course exercises
* Access to a charged fire hydrant
* Hydrant wrench, **NFES 0688**
* Reducer from hydrant threads to 1½” NH-M

50 each – traffic cones (actual number dependent upon course layout)

Field Exercise Supplies

These items need to be procured through established procurement channels or acquired through local fire cache.

* 5 rolls – ribbon, flagging, orange **NFES 2398**
* 10 lengths – 1½” x 100’ (1,000’ total) CJRL hose **NFES 0967**
* 5 lengths – 1” x 100’ (500’ total) CJRL hose **NFES 0966**
* 5 each – gated wye, 1½" **NFES 0231**
* 5 each – inline tee, 1½” **NFES 0230**
* 6 each – reducer, 1½” NH-F to 1” NPSH-M **NFES 0010**
* 3 each – 1½" combi-barrel nozzle **NFES 1082**
* 6 each – 1" combi-barrel nozzle **NFES 1081**
* 3 each – hose clamps **NFES 0046**
* 2 each – pressure relief valve **NFES 0229**
* 2 each – spanner wrench **NFES 0234**
* 2 each – collapsible 1,000 gallon tank **NFES 0588**
* 2 each – foot valve 1½" NH-F **NFES 0212**
* 2 each – foam nozzle 3/4" NH 8 GPM **NFES 0627**
* 2 each – foam nozzle 1½" NH 16 GPM **NFES 0628**
* 2 each – foam nozzle 1½" NH 30 GPM **NFES 0629**
* 4 pails – foam, Class A (20 gallons total) **NFES 1145**
* 1 package – Check-in List, ICS 211 **NFES 1335**
* 10 each – clipboard **NFES 0771**
* Hand-held radios
* Water tenders

Flow meters